|  |  |  |
| --- | --- | --- |
| Processed Image | Original Image | Text |
|  |  | How do WAN Edge devices operate when vSmart is inaccessible or fails to be reached by the WAN Edge? - © They cease to forward traffic in the data piane.  © They continue to receive reachability updates.  © They continue operating normally for a configurable time.  © They continue operation normally. |

|  |  |  |
| --- | --- | --- |
| Processed Image | Original Image | Text |
|  |  | How are policies deployed on cloud-hosted Cisco SD-WAN controllers? — © Policies are created on vSmart and enforced by vManage. © Policies are created on vManage and enforced by vSmart. © Policies are created on vManage and enforced by vManage. © Policies are created on vSmart and enforced by vSmart. |